**All MOBILE CODES**

**>>> SAMSUNG MOBILE CODES:- <<<**

**\*#1111# S/W Version
\*#1234# Firmware Version
\*#2222# H/W Version
\*#8999\*8376263# All Versions Together
\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\*#8999\*8378# Test Menu
\*#4777\*8665# GPSR Tool
\*#8999\*523# LCD Brightness
\*#8999\*377# Error Menu
\*#8999\*327# EEP Menu
\*#8999\*3825523# Don't Know.
\*#8999\*667# Debug Mode
\*#92782# PhoneModel (Wap)
#\*5737425# JAVA Mode
\*#2255# Call List
\*#232337# Bluetooth MAC Adress
\*#5282837# Java Version
\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

#\*4773# Incremental Redundancy
#\*7752# 8 PSK uplink capability bit
#\*7785# Reset wakeup & RTK timer cariables/variables
#\*1200# ?
#\*7200# Tone Generator Mute
#\*3888# BLUETOOTH Test mode
#\*#8999\*324# ??
#\*7828# Task screen
#\*5111# ??
#\*#8377466# S/W Version & H/W Version
#\*2562# Restarts Phone
#\*2565# No Blocking? General Defense.
#\*3353# General Defense, Code Erased.
#\*3837# Phone Hangs on White screen
#\*3849# Restarts Phone
#\*3851# Restarts Phone
#\*3876# Restarts Phone
#\*7222# Operation Typ: (Class C GSM)
#\*7224# !!! ERROR !!!
#\*7252# Operation Typ: (Class B GPRS)
#\*7271# CMD: (Not Available)
#\*7274# CMD: (Not Available)
#\*7337# Restarts Phone (Resets Wap Settings)
#\*2787# CRTP ON/OFF
#\*2886# AutoAnswer ON/OFF
\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

#\*3737# L1 AFC
#\*5133# L1 HO Data
#\*7288# GPRS Detached/Attached
#\*7287# GPRS Attached
#\*7666# White Screen
#\*7693# Sleep Deactivate/Activate
#\*7284# L1 HO Data
#\*2256# Calibration info? (For CMD set DEBUGAUTONOMY in cihard.opt)
#\*2286# Databattery
#\*2527# GPRS switching set to (Class 4, 8, 9, 10)
#\*2679# Copycat feature Activa/Deactivate
#\*3940# External looptest 9600 bps
#\*4263# Handsfree mode Activate/Deactivate
#\*4700# Please use function 2637
#\*7352# BVMC Reg value (LOW\_SWTOFF, NOMINAL\_SWTOFF)
#\*2558# Time ON
#\*3370# Same as 4700
#\*3941# External looptest 115200 bps
#\*5176# L1 Sleep
#\*7462# SIM Phase
#\*7983# Voltage/Freq
#\*7986# Voltage
#\*8466# Old Time
#\*2255# Call Failed
#\*5187# L1C2G trace Activate/Deactivate
#\*5376# DELETE ALL SMS!!!!
#\*6837# Official Software Version: (0003000016000702)
#\*7524# KCGPRS: (FF FF FF FF FF FF FF FF 07)
#\*7562# LOCI GPRS: (FF FF FF FF FF FF FF FF FF FF FF FE FF 01)
#\*2337# Permanent Registration Beep
\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

#\*2474# Charging Duration
#\*2834# Audio Path (Handsfree)
#\*3270# DCS Support Activate/Deactivate
#\*3282# Data Activate/Deactivate
#\*3476# EGSM Activate/Deactivate
#\*3676# FORMAT FLASH VOLUME!!!
#\*4760# GSM Activate/Deactivate
#\*4864# White Screen
#\*5171# L1P1
#\*5172# L1P2
#\*5173# L1P3
#\*7326# Accessory
#\*7683# Sleep variable
#\*8465# Time in L1
#\*2252# Current CAL
#\*2836# AVDDSS Management Activate/Deactivate
#\*3877# Dump of SPY trace
#\*7728# RSAV
#\*2677# Same as 4700
#\*3797# Blinks 3D030300 in RED
#\*3728# Time 2 Decod
#\*3725# B4 last off
#\*7372# Resetting the time to DPB variables
#\*7732# Packet flow context bit Activate/Deactivate
#\*6833# New uplink establishment Activate/Deactivate
#\*3273# EGPRS multislot (Class 4, 8, 9, 10)
#\*7722# RLC bitmap compression Activate/Deactivate
#\*2351# Blinks 1347E201 in RED
#\*4472# Hysteresis of serving cell: 3 dB
#\*2775# Switch to 2 inner speaker
#\*9270# Force WBS
#\*7878# FirstStartup (0=NO, 1=YES)
#\*3757# DSL UART speed set to (LOW, HIGH)
#\*8726# Switches USBACM to Normal
#\*8724# Switches USBACM to Generator mode
#\*8727# Switches USBACM to Slink mode
#\*8725# Switches USBACM to Loop-back mode
#\*3838# Blinks 3D030300 in RED
#\*2077# GPRS Switch
#\*2027# GPRS Switch
#\*0227# GPRS Switch
#\*0277# GPRS Switch
#\*22671# AMR REC START
#\*22672# Stop AMR REC (File name: /a/multimedia/sounds/voice list/ENGMODE.amr)
#\*22673# Pause REC
\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

#\*22674# Resume REC
#\*22675# AMR Playback
#\*22676# AMR Stop Play
#\*22677# Pause Play
#\*22678# Resume Play
#\*77261# PCM Rec Req
#\*77262# Stop PCM Rec
#\*77263# PCM Playback
#\*77264# PCM Stop Play
#\*2872# CNT
\*#8999\*283#
#\*22679# AMR Get Time
\*288666#
\*2886633#
\*#8999\*364# Watchdog ON/OFF
#\*8370# Tfs4.0 Test 0
#\*8371# Tfs4.0 Test 1
#\*8372# Tfs4.0 Test 2
#\*8373# Tfs4.0 Test 3
#\*8374# Tfs4.0 Test 4
#\*8375# Tfs4.0 Test 5
#\*8376# Tfs4.0 Test 6
#\*8377# Tfs4.0 Test 7
#\*8378# Tfs4.0 Test 8
#\*8379# Tfs4.0 Test 9
#837837# error=...
\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

#\*36245# Turns Email TestMenu on.

\*2767\*22236245# Email EPP set (....)!
\*2767\*837836245# Email Test Account!
\*2767\*29536245# Email Test2 Account!
\*2767\*036245# Email EPP reset!
\*2767\*136245# Email EPP set (1)!
\*2767\*736245# Email EPP set (7)!
\*2767\*3036245# Email...
\*2767\*3136245# Email...
\*2767\*3336245# Email...
\*2767\*3436245# Email...
\*2767\*3936245# Email...
\*2767\*4136245# Email...
\*2767\*4336245# Email...
\*2767\*4436245# Email...
\*2767\*4536245# Email...
\*2767\*4636245# Email...
\*2767\*4936245# Email...
\*2767\*6036245# Email...
\*2767\*6136245# Email...
\*2767\*6236245# Email...
\*2767\*6336245# Email...
\*2767\*6536245# Email...
\*2767\*6636245# Email...
\*2767\*8636245# Email...
\*2767\*85236245# Email...
\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\*2767\*3855# = E2P Full Reset
\*2767\*2878# = E2P Custom Reset
\*2767\*927# = E2P Wap Reset
\*2767\*226372# = E2P Camera Reset
\*2767\*688# Reset Mobile TV
#7263867# = RAM Dump (On or Off)
\*2767\*49927# = Germany WAP Settings
\*2767\*44927# = UK WAP Settings
\*2767\*31927# = Netherlands WAP Settings
\*2767\*420927# = Czech WAP Settings
\*2767\*43927# = Austria WAP Settings
\*2767\*39927# = Italy WAP Settings
\*2767\*33927# = France WAP Settings
\*2767\*351927# = Portugal WAP Settings
\*2767\*34927# = Spain WAP Settings
\*2767\*46927# = Sweden WAP Settings
\*2767\*380927# = Ukraine WAP Settings
\*2767\*7927# = Russia WAP Settings
\*2767\*30927# = GREECE WAP Settings
\*2767\*73738927# = WAP Settings Reset
\*2767\*49667# = Germany MMS Settings
\*2767\*44667# = UK MMS Settings
\*2767\*31667# = Netherlands MMS Settings
\*2767\*420667# = Czech MMS Settings
\*2767\*43667# = Austria MMS Settings
\*2767\*39667# = Italy MMS Settings
\*2767\*33667# = France MMS Settings
\*2767\*351667# = Portugal MMS Settings
\*2767\*34667# = Spain MMS Settings
\*2767\*46667# = Sweden MMS Settings
\*2767\*380667# = Ukraine MMS Settings
\*2767\*7667#. = Russia MMS Settings
\*2767\*30667# = GREECE MMS Settings**

Nokia mobile codes

**NOTE:> These Codings apply only for selected Nokia Mobile Phones...

>>Imp. Codes

 Blututh Dev Adrz
     \*#2820#

  Soft Frmt
   \*#7780#

  Hard Frmt
    \*#7370#

  Shw Vrsn
   \*#0000#

   IMEI
   \*#06#**

**>>CODES DESCRIPTIONS

\*3370# Activate Enhanced Full Rate Codec (EFR) - Your phone uses the best sound quality but talk time is reduced my approx. 5%

 #3370# Deactivate Enhanced Full Rate Codec (EFR)

 \*#4720# Activate Half Rate Codec - Your phone uses a lower quality sound but you should gain approx 30% more Talk Time

 \*#4720# Deactivate Half Rate Codec

 \*#0000# Displays your phones software version, 1st Line : software Version, 2nd Line : software Release Date, 3rd Line : Compression Type

 \*#9999# Phones software version if \*#0000# does not work

 \*#06# For checking the International Mobile Equipment Identity (IMEI Number)

 #pw+1234567890+1# Provider Lock Status. (use the "\*" button to obtain the "p,w" and "+" symbols)

 #pw+1234567890+2# Network Lock Status. (use the "\*" button to obtain the "p,w" and "+" symbols)

 #pw+1234567890+3# Country Lock Status. (use the "\*" button to obtain the "p,w" and "+" symbols)

 #pw+1234567890+4# SIM Card Lock Status. (use the "\*" button to obtain the "p,w" and "+" symbols)

 \*#147# (vodafone) this lets you know who called you last

 \*#1471# Last call (Only vodofone)

 \*#21# Allows you to check the number that "All Calls" are diverted to

 \*#2640# Displays security code in use

 \*#30# Lets you see the private number

 \*#43# Allows you to check the "Call Waiting" status of your phone.

 \*#61# Allows you to check the number that "On No Reply" calls are diverted to

 \*#62# Allows you to check the number that "Divert If Unreachable (no service)" calls are diverted to

 \*#67# Allows you to check the number that "On Busy Calls" are diverted to

 \*#67705646# Removes operator logo on 3310 & 3330

 \*#73# Reset phone timers and game scores

 \*#746025625# Displays the SIM Clock status, if your phone supports this power saving feature "SIM Clock Stop Allowed", it means you will get the best standby time possible

 \*#7760#  Manufactures code
\*#7780#  Restore factory settings
\*#8110#  Software version for the nokia 8110

 \*#92702689# Displays - 1.Serial Number, 2.Date Made, 3.Purchase Date, 4.Date of last repair (0000 for no repairs), 5.Transfer User Data. To exit this mode you need to switch your phone off then on again

\*#94870345123456789# Deactivate the PWM-Mem

 \*\*21\*number# Turn on "All Calls" diverting to the phone number entered

 \*\*61\*number# Turn on "No Reply" diverting to the phone number entered

 \*\*67\*number# Turn on "On Busy" diverting to the phone number entered

>> 12345 This is the default security code
press and hold # Lets you switch between lines

 \*#3283# or \*#DATE# Date of Manufacture
\*#682371158412125# Software Version**

### LG Mobile Codes

***NOTE:>> All Codings are depend on mobile versions......*

On the main screen type \*#06# For Information you get from the IMEI (International Mobile Equipment Identity)
XXXXXX XX XXXXXX X
TAC FAC SNR SP

TAC = Type approval code of your LG Mobile
FAC = Final assembly code of your cellphone
SNR = Serial number of your LG Phone
SP = Spare**

**>>Other secret tricks for LG mobile or cellphone

LG all models test mode:
Type 2945#\*# on the main screen.
2945\*#01\*# Secret menu for LG
IMEI and SW (LG 510): \*#07#
Software version (LG B1200): \*8375#
Recount cheksum (LG B1200): \*6861#
Factory test (B1200): #PWR 668
Simlock menu (LG B1200): 1945#\*5101#
Simlock menu (LG 510W, 5200): 2945#\*5101#
Simlock menu (LG 7020, 7010): 2945#\*70001#
Simlock menu (LG 500, 600): 2947#\*

LG-U81XX SPECIAL CODES
Code to read phone version :
- Phone without SIM
- Enter 277634#\*# or 47328545454#
- Select 'SW Ver.info'
Code to reset phone :
- Phone without SIM

- Enter 277634#\*# or 47328545454#
- Select 'Factory Reset'

Code to enter UNLOCK MENU :
- Phone wit SIM inside
- Enter 2945#\*88110#
Test Menu 8330 : 637664#\*#
Test Menu 8180 V10a: 49857465454#
Test Menu 8180 V11a: 492662464663#
Test Menu 8130-8138: 47328545454#
Test Menu 8110-8120: 277634#\***